GE21 Optohybrid Board Layout

**06/15/2018**

1. Note on the board (primary side):

**GE2/1 Optohybrid Board**

**Rice University, July 2018**

1. Board thickness 62 mil.
2. 8 (?) layers
3. Test points should be labeled on the primary side.
4. Differential pairs are marked with red circle on the schematic. Use guidelines below for routing. The length of pairs may vary (greatly simplifies the routing)

